{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":5,"n_cols":15,"rows_kept":5,"merged":[[0,0,0,14],[2,8,4,8],[2,10,4,10],[2,11,4,11],[2,12,4,12],[2,13,4,13]],"flags":["formulas_cached_only"]}
["甘煤一公司（王家山副立井项目部）2026年1月下旬所需物资（一标段）明细表"]
["物资编号","分类编码","物料分类","物资名称","规格型号","单位","数量","税率","技术要求及执行标准","品牌/厂家","进货日期","标段划分","付款形式及周期","使用单位","备注"]
[107,null,null,"焊管","外径48mm，壁厚3.5mm/L6m","m",150,{"v":0.13,"d":"13%"},"符合国家标准及行业标准","河北","中标后5日内送达","一标段","挂账后6个月内付清","甘肃煤炭第一工程有限责任公司矿建第六分公司王家山副立井项目部","含配套法兰盘及法兰垫"]
[108,null,null,"线材","φ10","吨",2,{"v":0.13,"d":"13%"},null,"酒钢\\兰鑫",{"$nulls":4},"HPB300型，1盘"]
[109,null,null,"螺纹钢","φ22mm，L=12m","吨",70,{"v":0.13,"d":"13%"},null,"酒钢\\宁钢",{"$nulls":4},"HRB400E（抗震性）分批进场 \n钢筋纵筋要直      "]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}